S100 OpenExplorer

# #hbUCPSchedParam

`typedef struct hbUCPSchedParam { int32_t priority; int64_t customId; uint64_t backend; uint32_t deviceId; } hbUCPSchedParam;`

Control parameter structure.

- Member

  Member Name | Description
  --- | ---
  `priority` | Task priority. For details, see hbUCPTaskPriority
  `customId` | Custom priority, e.g. timestamp, frame id, etc. The smaller the value, the higher the priority. Priority: priority > customId.
  `backend` | Task execution hardware, e.g. HB_UCP_BPU_CORE_0.
  `deviceId` | Device ID.

On This Page