S100 OpenExplorer

# #The hb_model_info Tool

The `hb_model_info` tool is used to parse the dependencies and parameters of the *.hbm, the *.bc in compilation and the basic information of the *.onnx model, at the same time support the checking of *.bc deletable nodes, and you can view the model structure by starting the webserver.

## #Support Range

It supports viewing the basic information of *.onnx models, the dependencies and parameters information of *.bc model, the information of deletable nodes, as well as the dependencies and parameters information of *.hbm model.

## #Usage

`Usage: hb_model_info [OPTIONS] MODEL_PATH A tool to get info about model compilation parameters, properties Options: -h, --help Show this message and exit. --version Show the version and exit. -v, --visualize Start netron server to show model structure`

## #Parameters Introduction

Parameter Name | Parameter Description
`-h, --help` | Display help information and exit.
`--version` | Display version information and exit.
`-v, --visualize` | Start netron server to view the model structure, you can close it with `Ctrl+C` when you finish viewing.

## #Usage Example

Taking the `resnet50_224x224_nv12.hbm` model as an example, you can refer to the following command to view the model compilation information:

`hb_model_info ./model_output/resnet50_224x224_nv12.hbm`

## #Output Contents

The output includes some input information during model compilation, as well as memory usage information occupied when the model is deployed and run on the board, as shown below:

Note

The version number information and other content in the following code block will change with the release package version, and here is only as an example.

`log will be stored in /open_explorer/samples/ai_toolchain/horizon_model_convert_sample/03_classification/03_resnet50/hb_model_info.log Start hb_model_info.... hb_model_info version 3.4.3 hbm_path: /open_explorer/samples/ai_toolchain/horizon_model_convert_sample/03_classification/03_resnet50/model_output/resnet50_224x224_nv12.hbm pid:94252 tid:94252 hbrt4_log/src/logger.rs:402: Logger of HBRT4 initialized, version = 4.4.3 pid:94252 tid:94252 hbrt4_loader/src/parsing.rs:91: Load hbm from file; filename="resnet50_224x224_nv12.hbm" pid:94361 tid:94361 hbrt4_log/src/logger.rs:402: Logger of HBRT4 initialized, version = 4.4.3 pid:94361 tid:94361 hbrt4_loader/src/parsing.rs:42: Load hbm header from file; filename="resnet50_224x224_nv12.hbm" pid:94361 tid:94361 hbrt4_log/src/logger.rs:402: Logger of HBRT4 initialized, version = 4.4.3 pid:94361 tid:94361 hbrt4_loader/src/parsing.rs:91: Load hbm from file; filename="resnet50_224x224_nv12.hbm" FPS=1145.9400000000001, latency = 872.60000000000002 us, DDR = 26316800 bytes, Compiling HBDK version = "4.4.3" (see .hb_model_info/resnet50_224x224_nv12.html) HBDK hbm perf SUCCESS ************* resnet50_224x224_nv12 ************* ############# model deps info ############# builder version : 3.4.3 hbdk version : 4.4.3 hmct version : 2.0.5 ############# model_parameters info ############# onnx_model : /open_explorer/samples/ai_toolchain/horizon_model_convert_sample/01_common/model_zoo/mapper/classification/resnet50/resnet50.onnx BPU march : nash-e layer_out_dump : False working dir : /open_explorer/samples/ai_toolchain/horizon_model_convert_sample/03_classification/03_resnet50/model_output output_model_file_prefix: resnet50_224x224_nv12 node_info : {} ############# input_parameters info ############# ------------------------------------------ ---------input info : input --------- input_name : input input_type_rt : nv12 input_space&range : regular input_type_train : rgb input_layout_train : NCHW norm_type : data_mean_and_scale input_shape : 1x3x224x224 mean_value : [123.675, 116.28, 103.53] scale_value : [0.01712475, 0.017507, 0.01742919] std_value : [] separate_batch : False ---------input info : input end ------- ------------------------------------------ ############# calibration_parameters info ############# calibration_type : default max_percentile : None per_channel : False cal_data_dir : /open_explorer/samples/ai_toolchain/horizon_model_convert_sample/03_classification/03_resnet50/calibration_data_rgb ############# compiler_parameters info ############# debug : True optimize_level : O2 compile_mode : latency core_num : 1 balance_factor : 100 input_source : {'input': 'pyramid'} cache_mode : disable ############# memory info ############# input memory : 75264 output memory : 4096 static memory : 26478248 dynamic memory : 79360 intermediate memory : 0 temporary memory : 0 min memory requirement: 26557608 hbm_path: /open_explorer/samples/ai_toolchain/horizon_model_convert_sample/03_classification/03_resnet50/model_output/resnet50_224x224_nv12.hbm pid:94252 tid:94252 hbrt4_loader/src/parsing.rs:42: Load hbm header from file; filename="resnet50_224x224_nv12.hbm" pid:94252 tid:94252 hbrt4_log/src/logger.rs:402: Logger of HBRT4 initialized, version = 4.4.3 pid:94252 tid:94252 hbrt4_loader/src/parsing.rs:91: Load hbm from file; filename="resnet50_224x224_nv12.hbm" ############# Model input/output info ############# NAME TYPE SHAPE DATA_TYPE ------ ------ ---------------- --------- input_y input [1, 224, 224, 1] UINT8 input_uv input [1, 112, 112, 2] UINT8 output output [1, 1000] FLOAT32`
On This Page